1. Cross River Rail is a proposed north-south rail line in Brisbane’s inner city, including a new tunnel under the Brisbane River and new underground inner city rail stations.

1. Following technical investigations and community and stakeholder consultation, the Cross River Rail reference design was developed which includes tunnel design, surface track design, station design and entry points, property requirements and construction sites.
2. The reference design is divided into three sections:
* 9.8km two track tunnel between Yeerongpilly train station through to the Exhibition line in Victoria Park
* 5km of two additional surface tracks from the southern portal at Yeerongpilly to south of Salisbury junction
* 3km of 2 additional surface tracks on the Exhibition loop from the northern portal at Victoria Park to Breakfast Creek
1. Cabinet approved the release of the reference design for Cross River Rail for public consultation.
2. *Attachments*
* [Cross River Rail Reference Design](Attachments/pdf_cross_river_rail_reference_design_overview%5B1%5D.pdf)